**Section 1: Chemical Product and Company Identification**

Product Identification : Humidity Absorbent

Distributor & Manufacturer : Azadi Co., Ltd

Address : 518 To Ngoc Van Street, Tam Binh Ward, Thu Duc City,

Ho Chi Minh City, Viet Nam

Phone/Fax : +084-089 6161 666

Trade Name : Azadi Power Desiccant

Chemical Family : Salt, Polyester, Polyethylene, Starch

**Section 2: Composition/ Information of Ingredients**

|  |  |
| --- | --- |
| Chemical Name | CAS # |
| Polyester bag, Polyethylene Bag | 9002-88-4 |
| Calcium Chloride | 10043-52-4 |
| Modified Starch | 9005-25-8 |
| Carbon Active | 7440-44-0 |
| Carbonate Salt | 144-55-8 |
| Nonwoven Membrane | 9007-88-4 |

**Section 3: Hazard Identification**

Physical state : package powder desiccant, changes to gel when saturated.

General Health Effect : No health hazard in normal industrial use. However, health hazards do exist as a result of the dust generated if the container is cut, split or otherwise compromised. Prolonged or excessive exposure to dust may cause lung damage. Dust can be irritating to eyes and skin.

Potential Health Effect : This material is normally packaged and contained in a bag and wrapped by plastic. If the plastic and bag are opened, prolonged or repeated inhalation of the dust may cause irritating to respiratory tracts.

Carcinogenic information : none of the components present in this material at concentration is equal to or greater than 0.1% as listed by IARC, NTP, OSHA or ACGIH as a carcinogen.

**Section 4: First Aid Measures**

Eye Contact : mechanical irritation-remove particle. Seek medical help if irritation persists.

Skin contact : wash skin with water and soap

Ingestion : normally not needed. If large quantities are ingested, seek medical advice.

Inhalation : remove immediately to fresh air. Seek medical attention if cough or other symptoms develop or persist.

In case of inhalation : in case of adverse exposure to vapors and/or aerosols formed at elevated temperatures, immediately remove the effected victim from exposure. Administer artificial respiration if breathing is stopped. Keep at rest. Call for prompt medical attention.

In case of skin contact : for hot product ( molten product), immediately immerse in or flush affected area with large amounts of cold water to dissipate heat. Use soap if necessary. Seek medical attention if effects persist. Cover with clean cotton sheeting or gauze and get prompt medical attention. No attempt should be made to remove material from skin or to remove contaminated clothing

**Section 5: Fire Fighting Measures**

Flash point (method) : N/A (above 600**°**F, estimated)

Auto ignition temperature : N/A (> 600**°**F estimated)

Explosive : N/A

Lower explosion limit : N/A

Upper explosion limit : N/A

Flammability class : N/A

Extinguishing media : Use extinguishing agent applicable to surrounding fire Use water fog, foam, dry chemical or CO2

Hazardous combustion : N/A

Hazardous Decomposition : Carbon Monoxide, Carbon Dioxide

Incompatibility : Avoid excessive heat, avoid strong oxidizers, caustics and Fluorines.

Unusual fire and explosion hazard : Treat as soil that can burn. Molded part generally burns with a low smoke density and dripping flame.

Fire-fighting instructions/equipment : As in any fire, wear self-contained breathing apparatus operated by pressure-demand mode and full protective gear.

Special Fire Fighting : Standard procedures for Class A fires.

Material will not burn unless preheated. Do not enter confined fire area without full bunker gear (helmet with face shield, bunker coats, gloves rubber boats), respiratory (including positive pressure NIOSH/MSHA approved self-container breathing apparatus) and eye protection required for fired fighting personnel. Use water spray to cool exposed surfaces and to protect personnel. Isolate “fuel” supply from fire. Extinguish the fire by cooling with water spray.

**Section 6: Accidental Release Measures**

Safeguards ( Personnel ) : Do not inhale if conditions are dusty and use appropriate gloves.

Spill clean up : Collect in suitable containers for recovery or disposal.

Containment produces : Pick up large pieces. Flush residual with plenty of water.

**Section 7: Accidental Release Measures**

Handling : Use of proper hygiene practices when handling product in workplace. Wash hands after handling and before eating. Keep away from the eyes.

Storage : Store in dry area and do not open outer plastic bag before use as it will become activate. Do not store near flame, or heat or strong oxidants such as hot or concentrated nitric acid or fuming sulfuric acid.

**Section 8: Exposure Controls/ Personal Protection**

Personal Protective Equipment

Eye/face : None needed during normal use and handling

Respirator : None needed during normal use and handling

Protective gloves : None needed during normal use and handling

Exposure Guidelines

Applicable Exposure Limits : OSHA HAZARDOUS COMPONENTS

**Section 9: Physical and Chemical Properties**

Physical Data

Boiling point : N/A Specific gravity : N/A

Melting point : N/A Vapor Density (AIR=1) : N/A

Solubility : Insoluble

Odor : Odorless

Form : Bag

**Section 10: Stability and Reactivity**

Chemical Stability : Stable

Polymerization : Polymerization will not occur

Incompatibility : Strong oxidizing agents, fluorine

**Section 11: Toxicological Information**

Carcinogenicity : N/A NTP : N/A

Sensitization : Not sensitizing

Acute toxicity : None identified

**Section 12: Ecological Information**

Ecotoxicological Information

Non-toxic-insoluble

This material is part of mineral origin. It is not biodegradable.

**Section 13: Disposal Consideration**

Waste Disposal : cut open the bag, empty the contents into suitable containers and dispose of the contents as organic waste. The polyethylene and polypropylene bag is recyclable but maybe disposed of as industrial waste by an approved contractor.

**Section 14: Transportation Information**

Shipping Information

DOT Shipping Name: This product is not classified as hazardous for transportation, by air, sea and road freight.

**Section 15: Regulatory Information**

IKEA Specification IOS-MAT-0010 On Total Lead Content :Pass

IKEA Specification IOS-MAT-0010 On Total Cadmium Content : Pass

IKEA Specification IOS-MAT-0010 On Organo Tin Content : Pass

U.S. 21 CFR F.D.A. Regulation Part 177.1520 Clause 3.1a And 3.1b for Olefin Copolymer : Pass

*Polyester Bag( Polyethylene Bag):*

SARA 311/312: This product is not classified as hazardous under SARA 311/312

None of this product’s components are listed under SARA 302 (40 CFR 355 Appendix A), SARA section 313( 40 CFR 372.65) or CERCLA (40 CFR 302.4)

*Modified Starch:*

WHMIS : Not controlled

Canadian Domestic Substance List (DSL) : On inventory

*PE&PP Membrane:*

There are two components in here. Both of them are Plastic. Both of them are recyclable so they can be put in the plastic waste only. It doesn’t need to separate them.

If thermally decomposed, flammable/toxic gases may be released. Upon combustion with insufficient air, carbon monoxide and gaseous hydrocarbons may be generated.

Incinerating PE&PP Membrane requires temperatures about 30**°C** to produce smoke and combustible gases. Material will not burn unless preheated. Do not enter confined fire spa without full bunker gear( helmet with face shield, bunker coats, gloves rubber boats), respiratory( including positive pressure NIOSH approved self-container breathing apparatus) and eye protection required for fire fighting personnel. Use water spray to cool fire exposed surfaces and to protect personnel. Isolate “fuel” supply to fire. Extinguish the fire by cooling with water spray.

*Calcium Chloride:*

UNITED STATES

SARA TITLE III ( SUPERFUND AMENDMENTS AND REAUTHORIZATION ACT)

Fire : No; Pressure generating: No; Reactivity: No; Acute: Yes;

Chronic: No

311/312 hazard categories: does not meet any hazard categories

Title III Notes: This product contains no substances which are defined as toxic chemical under the reporting requirements of section 313 of Title III of Superfund Amendments And Reauthorization Act of 1986

**Section 16: Other Information**

Reason for issue : Annual review

Revised date : September 01, 2022

Revision # : none